{"text_format":"3","workbook":"xlsb","n_sheets":1,"sheets":["OEM Products"],"not_rendered":{"external_links":1,"defined_names":3},"read":"bin_record_odd","date_system":"1900","formulas":"cached_only","passed_over":{"ids":[37,38,1024],"n":72}}

{"sheet":"OEM Products","index":0,"n_rows":19,"n_cols":66,"rows_kept":19,"merged":[[1,1,1,33],[2,34,2,65]],"read":"bin_record_odd","flags":["formulas_cached_only"]}
[null,"Last Update 09/23/2013"]
[null,"Opticon - OEM Product Matrix"]
[{"$nulls":34},"Symbologies"]
["Product","     1D Symbol Decoding \n      (*requires decoder)","     2D Symbol Decoding","Decoded/Undecoded","Decoder Board","Scan Technology","     Imager Technology","     Power Voltage (Typ.)","     Current (Power Off Mode)","Current (Sleep Mode - Typ)","Current ( Idle Mode - Typ)","Current Operating (Typ)","     Current  (Peak - Max)","     Product Market","       GoodRead LED Output","       Beeper Output","     Ext. Illumination Cntrl Output","     AIMing Input","Aiming Method","Illumination Source","Laser/LED Class","Image Sensor Size","Shutter technology","     Focus","Field of View (H x V)\nLaser (readable) Scan Width (H)","     Scans Per Second","     Frames Per Second","       BAR/SPACE Signal Output","       232 Serial CMOS","       USB-HID (Keyboard I/F)","       USB-Virtual COM Port","     FFC Connector Size (contacts)","  Apx Size mm (W-xHxD)\n    * Camera Sensor Only","Density","      JAN/UPC/EAN (8,13,addon)","      Codabar / NW-7","      Code 11","      Code 39","      Code 93","      Code 128","      GS1-128 (EAN-128)","      GS1 - Databar (RSS)","       IATA","      Industrial 2/5","      Interleaved 2/5","       Matrix 2/5","      MSI/Plessey","      UK/Plessey","      S-Code","      Telepen","       Tri-Optic","      ISBN / ISSN / ISMN","      Postal - Chinese Post","     Postal - Korean Post Auth.","     Postal - Intelligent Barcode","     Postal - POSTNET","     Composite Codes","      PDF417","       Micro PDF417","       Codablock F","       Data Matrix ","       Aztec","       Chinese Sensible Code","       QR Code","       Micro QR Code","      Maxicode"]
["MDI1000","YES","YES","Decoded","Separate","Imager","CMOS","3.3V","N/A","25mA","125mA","310mA","410mA","OEM","Y","Y","Y","Y","2 GRN LEDs","4 Red LEDs","Class 1","1280x1024","Rolling","120mm","47° x 38°","N/A","30","N","Y","N","Y","30","*22x12x14","Standard","Y","Y","N","Y","Y","Y","N","Y","Y","Y","Y","N","Y","N","N","N","N","N","N","N","N","N","Y","Y","Y","N","Y","Y","N","Y","Y","Y"]
["MDI1002","YES","YES","Decoded","Separate","Imager","CMOS","3.3V","N/A","25mA","125mA","310mA","410mA","OEM","Y","Y","Y","Y","2 GRN LEDs","4 Red LEDs","Class 1","1280x1024","Rolling","60mm","47° x 38°","N/A","30","N","Y","N","Y","30","*22x12x14","High","Y","Y","N","Y","Y","Y","N","Y","Y","Y","Y","N","Y","N","N","N","N","N","N","N","N","N","Y","Y","Y","N","Y","Y","N","Y","Y","Y"]
["MDI2000","YES","YES","Decoded","Separate","Imager","CMOS","3.3V","N/A","15mA","70mA","240mA","300mA","OEM","N","N","N","Y","Laser Spot","1 Red LED","Class 2","900x512","Rolling","AUTO","43° x 23°","N/A","80","N","Y","N","Y","14","*27x14x13","Variable","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["MDI2300","YES","YES","Decoded","Separate","Imager","CMOS","3.3V","N/A","15mA","70mA","240mA","390mA","OEM","Y","Y","Y","Y","Laser Spot","1 Red LED","Class 1","900x512","Rolling","AUTO","43° x 23°","N/A","80","N","Y","Y","Y","17","*27x14x13","Variable","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["MDI2350","YES","YES","Decoded","Separate","Imager","CMOS","3.3V","N/A","15mA","70mA","240mA","300mA","OEM","Y","Y","Y","Y","Laser Spot","1 Red LED","Class 1","1280x1024","Rolling","120mm","47° x 38°","N/A","30","N","Y","Y","Y","17","*27x14x13","Standard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["MDI3000-SR","YES","YES","Decoded","Separate","Imager","CMOS","3-5.5V","<20uA","0.2mA","45mA","230mA","330mA","OEM","Y","Y","N","Y","Green LED","Amber LED","Class 1","752x480","Global","130mm","41° x 26°","N/A","60","N","Y","N","N","12","*22x12x14","Standard"]
["MDI3100-SR","YES","YES","Decoded","Integrated","Imager","CMOS","3-5.5V","<20uA","0.2mA","45mA","230mA","330mA","OEM","Y","Y","N","Y","Green LED","Amber LED","Class 1","752x480","Global","130mm","41° x 26°","N/A","60","N","Y","Y","Y","12","25x12x21","Standard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["MDI3100-HD","YES","YES","Decoded","Integrated","Imager","CMOS","3-5.5V","<20uA","0.2mA","45mA","230mA","330mA","OEM","Y","Y","N","Y","Green LED","Amber LED","Class 1","752x480","Global","70mm","41° x 26°","N/A","60","N","Y","Y","Y","12","25x12x21","High","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["MDL1000","YES","No","Decoded","Integrated","Laser","N/A","3.3V","N/A","<2mA","30mA","110mA","125mA","OEM","Y","Y","N","Y","Laser Spot","Laser","Class 2","N/A","N/A","N/A","44°","100","N/A","N","Y","N","N","12","28x8x18","Standard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","N","Y","Y","Y","Y","Y","Y","N","N","Y","Y","Y","N","N","N","N","N","N","N"]
["MDL2001","YES","No","Decoded","Integrated","Laser","N/A","3.3V","N/A","<2mA","30mA","110mA","125mA","OEM","Y","Y","N","Y","Laser Spot","Laser","Class 2","N/A","N/A","N/A","44°","100","N/A","N","Y","N","N","12","20x11x18","Standard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","N","N","Y","Y","Y","N","N","N","N","N","N","N"]
["MDL4000R1","YES","No","Decoded","Integrated","Laser","N/A","3.3V","N/A","<0.5mA","40mA","85mA","125mA","OEM","Y","Y","N","Y","Laser Spot","Laser","Class 1","N/A","N/A","N/A","44°","100","N/A","N","Y","N","N","12","20x14x6","Standard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","N","N","Y","Y","Y","N","N","N","N","N","N","N"]
["MDL4000U1","YES","No","Decoded","Integrated","Laser","N/A","3.3V","N/A","<0.5mA","40mA","85mA","125mA","OEM","Y","Y","N","Y","Laser Spot","Laser","Class 1","N/A","N/A","N/A","44°","100","N/A","N","N","Y","Y","12","20x14x6","Standard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","N","N","Y","Y","Y","N","N","N","N","N","N","N"]
["MSL1000","YES*","No","Undecoded","None","Laser","N/A","3.3V","N/A","<1uA","35mA","55mA","75mA","OEM","N","N","N","N","Laser Spot","Laser","Class 2","N/A","N/A","N/A","44°","100","N/A","Y","N","N","N","10","28x8x14","Standard","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N"]
["MSL2001","YES*","No","Undecoded","None","Laser","N/A","3.3V","N/A","<1uA","35mA","55mA","75mA","OEM","N","N","N","N","Laser Spot","Laser","Class 2","N/A","N/A","N/A","44°","100","N/A","Y","N","N","N","10","20x11x18","Standard","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N","N"]
[{"$nulls":10},"{Typ. currents w/default settings}"]